BOSST TECHNICAL PURPOSE

BEÑAT, JON, ABDE AND MIKEL

INDEX

[Machines and configuration: 2](#_Toc71274412)

# Machines and configuration:

In order to complete thin project we have two type o machines:

* Ubuntu server
* Windows client

In those machines, there are different configurations. Our Ubuntu has accommodated our web page, a mariadb server, phpmyadmin and webmin.

This machine has two different ip:

* WAN: DHCP.
* LAN: 204.204.5.1/24

The windows 10 is going to be the accountant’s pc. Therefore, in this pc there will be the java application. Moreover, this pc would connect to the server in order to change the configuration. This pc has also two Ethernet adapters:

* Eth1: DHCP
* Eth2: 204.204.5.12/24

This is how the local network is placed:

